Table 1: Characteristics of bridge circuit

|  |  |
| --- | --- |
| Property | Value |
| Analog input voltage range | 0 V to 5 V |
| Analog input resolution | 1024 |
| Analog output type | Pulse width modulation (PWM) |
| Analog output voltage range | 0 V to 5 V |
| Analog output resolution | 256 |
| Baud rate for RS232 protocol | 115, 200 bit/s |